<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<packages>
<package name="ARDUINO_UNO">
<description>Footprint for representing an Arduino Uno board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
</packages>
<symbols>
<symbol name="ARDUINO_UNO">
<description>Schematic symbol for representing an Arduino Uno board in an EAGLE schematic.
Created by Dave Young for Element14.  More EAGLE documentation at:
http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<pin name="28(SCL)"/>
<pin name="27(SDA)"/>
<pin name="AREF"/>
<pin name="GND"/>
<pin name="13"/>
<pin name="12"/>
<pin name="~11"/>
<pin name="~10"/>
<pin name="~9"/>
<pin name="8"/>
<pin name="7"/>
<pin name="~6"/>
<pin name="~5"/>
<pin name="4"/>
<pin name="~3"/>
<pin name="2"/>
<pin name="1(TX)"/>
<pin name="0(RX)"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN"/>
<pin name="GND."/>
<pin name="GND.."/>
<pin name="5V"/>
<pin name="3.3V"/>
<pin name="RESET"/>
<pin name="IOREF"/>
<pin name="(N/C)"/>
<pin name="&lt;PWR&gt;-V"/>
<pin name="&lt;PWR&gt;+V"/>
<pin name="&lt;USB&gt;GND"/>
<pin name="&lt;USB&gt;D-"/>
<pin name="&lt;USB&gt;D+"/>
<pin name="&lt;USB&gt;+V"/>
<pin name="+5V"/>
<pin name="MOSI"/>
<pin name="GND_"/>
<pin name="RESET."/>
<pin name="SCK"/>
<pin name="MISO"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ARDUINO_UNO" prefix="PCB">
<description>Device for representing an Arduino Uno board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_UNO"/>
</gates>
<devices>
<device name="" package="ARDUINO_UNO">
<connects>
<connect gate="G$1" pin="(N/C)" pad="N/C"/>
<connect gate="G$1" pin="+5V" pad="+5V"/>
<connect gate="G$1" pin="0(RX)" pad="0"/>
<connect gate="G$1" pin="1(TX)" pad="1"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="27(SDA)" pad="SDA"/>
<connect gate="G$1" pin="28(SCL)" pad="SCL"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="&lt;PWR&gt;+V" pad="&lt;PWR&gt;+V"/>
<connect gate="G$1" pin="&lt;PWR&gt;-V" pad="&lt;PWR&gt;-V"/>
<connect gate="G$1" pin="&lt;USB&gt;+V" pad="&lt;USB&gt;+V"/>
<connect gate="G$1" pin="&lt;USB&gt;D+" pad="&lt;USB&gt;D+"/>
<connect gate="G$1" pin="&lt;USB&gt;D-" pad="&lt;USB&gt;D-"/>
<connect gate="G$1" pin="&lt;USB&gt;GND" pad="&lt;USB&gt;GND"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND." pad="GND."/>
<connect gate="G$1" pin="GND.." pad="GND.."/>
<connect gate="G$1" pin="GND_" pad="GND_"/>
<connect gate="G$1" pin="IOREF" pad="I/OREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="RESET." pad="RESET."/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="~10" pad="10"/>
<connect gate="G$1" pin="~11" pad="11"/>
<connect gate="G$1" pin="~3" pad="3"/>
<connect gate="G$1" pin="~5" pad="5"/>
<connect gate="G$1" pin="~6" pad="6"/>
<connect gate="G$1" pin="~9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
