(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)

  (general
    (links 91)
    (no_connects 65)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 0)
    (tracks 78)
    (zones 0)
    (modules 46)
    (nets 83)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF5F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(ARD1-PadRST2)")
  (net 2 "Net-(ARD1-PadGND4)")
  (net 3 "Net-(ARD1-PadMOSI)")
  (net 4 "Net-(ARD1-PadSCK)")
  (net 5 "Net-(ARD1-Pad5V2)")
  (net 6 "Net-(ARD1-PadA0)")
  (net 7 "Net-(ARD1-PadVIN)")
  (net 8 GND)
  (net 9 VCC)
  (net 10 "Net-(ARD1-Pad3.3V)")
  (net 11 "Net-(ARD1-PadRST1)")
  (net 12 "Net-(ARD1-PadIORF)")
  (net 13 "Net-(ARD1-PadD0)")
  (net 14 "Net-(ARD1-PadD1)")
  (net 15 "Net-(ARD1-PadD2)")
  (net 16 "Net-(ARD1-PadD3)")
  (net 17 "Net-(ARD1-PadD4)")
  (net 18 "Net-(ARD1-PadD5)")
  (net 19 "Net-(ARD1-PadD6)")
  (net 20 "Net-(ARD1-PadD7)")
  (net 21 "Net-(ARD1-PadD8)")
  (net 22 "Net-(ARD1-PadD9)")
  (net 23 "Net-(ARD1-PadD10)")
  (net 24 "Net-(ARD1-PadSCL)")
  (net 25 "Net-(ARD1-PadSDA)")
  (net 26 "Net-(ARD1-PadAREF)")
  (net 27 "Net-(ARD1-PadD13)")
  (net 28 "Net-(ARD1-PadD12)")
  (net 29 "Net-(ARD1-PadD11)")
  (net 30 "Net-(ARD1-PadA1)")
  (net 31 "Net-(ARD1-PadA2)")
  (net 32 "Net-(ARD1-PadA3)")
  (net 33 "Net-(ARD1-PadA4)")
  (net 34 "Net-(ARD1-PadA5)")
  (net 35 "Net-(ARD1-PadMISO)")
  (net 36 "Net-(D1-Pad2)")
  (net 37 "Net-(D2-Pad2)")
  (net 38 "Net-(D3-Pad2)")
  (net 39 "Net-(D4-Pad2)")
  (net 40 "Net-(D5-Pad2)")
  (net 41 "Net-(D6-Pad2)")
  (net 42 "Net-(D7-Pad2)")
  (net 43 "Net-(D8-Pad2)")
  (net 44 "Net-(D9-Pad2)")
  (net 45 "Net-(D10-Pad2)")
  (net 46 "Net-(D11-Pad2)")
  (net 47 "Net-(D12-Pad2)")
  (net 48 "Net-(D13-Pad2)")
  (net 49 "Net-(D14-Pad2)")
  (net 50 "Net-(D15-Pad2)")
  (net 51 "Net-(D16-Pad2)")
  (net 52 "Net-(D17-Pad2)")
  (net 53 "Net-(D18-Pad2)")
  (net 54 "Net-(D19-Pad2)")
  (net 55 "Net-(D20-Pad2)")
  (net 56 "Net-(R1-Pad2)")
  (net 57 "Net-(R2-Pad2)")
  (net 58 "Net-(R3-Pad2)")
  (net 59 "Net-(R4-Pad2)")
  (net 60 "Net-(R5-Pad2)")
  (net 61 "Net-(R6-Pad2)")
  (net 62 "Net-(R7-Pad2)")
  (net 63 "Net-(R8-Pad2)")
  (net 64 "Net-(R9-Pad2)")
  (net 65 "Net-(R10-Pad2)")
  (net 66 "Net-(R11-Pad2)")
  (net 67 "Net-(R12-Pad2)")
  (net 68 "Net-(R13-Pad2)")
  (net 69 "Net-(R14-Pad2)")
  (net 70 "Net-(R15-Pad2)")
  (net 71 "Net-(R16-Pad2)")
  (net 72 "Net-(R17-Pad2)")
  (net 73 "Net-(R18-Pad2)")
  (net 74 "Net-(R19-Pad2)")
  (net 75 "Net-(R20-Pad2)")
  (net 76 "Net-(U1-Pad6)")
  (net 77 "Net-(U1-Pad7)")
  (net 78 "Net-(U1-Pad9)")
  (net 79 "Net-(U2-Pad7)")
  (net 80 "Net-(U2-Pad9)")
  (net 81 "Net-(U3-Pad7)")
  (net 82 "Net-(U3-Pad9)")

  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(ARD1-Pad3.3V)")
    (add_net "Net-(ARD1-Pad5V2)")
    (add_net "Net-(ARD1-PadA0)")
    (add_net "Net-(ARD1-PadA1)")
    (add_net "Net-(ARD1-PadA2)")
    (add_net "Net-(ARD1-PadA3)")
    (add_net "Net-(ARD1-PadA4)")
    (add_net "Net-(ARD1-PadA5)")
    (add_net "Net-(ARD1-PadAREF)")
    (add_net "Net-(ARD1-PadD0)")
    (add_net "Net-(ARD1-PadD1)")
    (add_net "Net-(ARD1-PadD10)")
    (add_net "Net-(ARD1-PadD11)")
    (add_net "Net-(ARD1-PadD12)")
    (add_net "Net-(ARD1-PadD13)")
    (add_net "Net-(ARD1-PadD2)")
    (add_net "Net-(ARD1-PadD3)")
    (add_net "Net-(ARD1-PadD4)")
    (add_net "Net-(ARD1-PadD5)")
    (add_net "Net-(ARD1-PadD6)")
    (add_net "Net-(ARD1-PadD7)")
    (add_net "Net-(ARD1-PadD8)")
    (add_net "Net-(ARD1-PadD9)")
    (add_net "Net-(ARD1-PadGND4)")
    (add_net "Net-(ARD1-PadIORF)")
    (add_net "Net-(ARD1-PadMISO)")
    (add_net "Net-(ARD1-PadMOSI)")
    (add_net "Net-(ARD1-PadRST1)")
    (add_net "Net-(ARD1-PadRST2)")
    (add_net "Net-(ARD1-PadSCK)")
    (add_net "Net-(ARD1-PadSCL)")
    (add_net "Net-(ARD1-PadSDA)")
    (add_net "Net-(ARD1-PadVIN)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D19-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D20-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad9)")
    (add_net VCC)
  )

  (module Arduino:Arduino_Uno_Shield (layer F.Cu) (tedit 5898A1DC) (tstamp 59B7E974)
    (at 57.15 135.89)
    (path /59B7F85C)
    (fp_text reference ARD1 (at 2.54 -54.356) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Arduino_Uno_Shield (at 15.494 -54.356) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 9.525 -32.385) (end -6.35 -32.385) (layer B.CrtYd) (width 0.15))
    (fp_line (start 9.525 -43.815) (end -6.35 -43.815) (layer B.CrtYd) (width 0.15))
    (fp_line (start 9.525 -43.815) (end 9.525 -32.385) (layer B.CrtYd) (width 0.15))
    (fp_line (start -6.35 -43.815) (end -6.35 -32.385) (layer B.CrtYd) (width 0.15))
    (fp_text user . (at 62.484 -32.004) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.43 -12.065) (end 11.43 -3.175) (layer B.CrtYd) (width 0.15))
    (fp_line (start -1.905 -3.175) (end 11.43 -3.175) (layer B.CrtYd) (width 0.15))
    (fp_line (start -1.905 -12.065) (end -1.905 -3.175) (layer B.CrtYd) (width 0.15))
    (fp_line (start -1.905 -12.065) (end 11.43 -12.065) (layer B.CrtYd) (width 0.15))
    (fp_line (start 0 -53.34) (end 0 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 66.04 -40.64) (end 66.04 -51.816) (layer F.SilkS) (width 0.15))
    (fp_line (start 68.58 -38.1) (end 66.04 -40.64) (layer F.SilkS) (width 0.15))
    (fp_line (start 68.58 -3.81) (end 68.58 -38.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 66.04 -1.27) (end 68.58 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 66.04 0) (end 66.04 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 64.516 -53.34) (end 66.04 -51.816) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 0) (end 66.04 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -53.34) (end 64.516 -53.34) (layer F.SilkS) (width 0.15))
    (pad RST2 thru_hole oval (at 63.627 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(ARD1-PadRST2)"))
    (pad GND4 thru_hole oval (at 66.167 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(ARD1-PadGND4)"))
    (pad MOSI thru_hole oval (at 66.167 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(ARD1-PadMOSI)"))
    (pad SCK thru_hole oval (at 63.627 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(ARD1-PadSCK)"))
    (pad 5V2 thru_hole oval (at 66.167 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(ARD1-Pad5V2)"))
    (pad A0 thru_hole oval (at 50.8 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(ARD1-PadA0)"))
    (pad VIN thru_hole oval (at 45.72 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(ARD1-PadVIN)"))
    (pad GND3 thru_hole oval (at 43.18 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad GND2 thru_hole oval (at 40.64 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 5V1 thru_hole oval (at 38.1 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 3.3V thru_hole oval (at 35.56 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(ARD1-Pad3.3V)"))
    (pad RST1 thru_hole oval (at 33.02 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(ARD1-PadRST1)"))
    (pad IORF thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(ARD1-PadIORF)"))
    (pad D0 thru_hole oval (at 63.5 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(ARD1-PadD0)"))
    (pad D1 thru_hole oval (at 60.96 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(ARD1-PadD1)"))
    (pad D2 thru_hole oval (at 58.42 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(ARD1-PadD2)"))
    (pad D3 thru_hole oval (at 55.88 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(ARD1-PadD3)"))
    (pad D4 thru_hole oval (at 53.34 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(ARD1-PadD4)"))
    (pad D5 thru_hole oval (at 50.8 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(ARD1-PadD5)"))
    (pad D6 thru_hole oval (at 48.26 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(ARD1-PadD6)"))
    (pad D7 thru_hole oval (at 45.72 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(ARD1-PadD7)"))
    (pad GND1 thru_hole oval (at 26.416 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad D8 thru_hole oval (at 41.656 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(ARD1-PadD8)"))
    (pad D9 thru_hole oval (at 39.116 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(ARD1-PadD9)"))
    (pad D10 thru_hole oval (at 36.576 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(ARD1-PadD10)"))
    (pad "" np_thru_hole circle (at 66.04 -7.62) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 66.04 -35.56) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 15.24 -50.8) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 13.97 -2.54) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad SCL thru_hole oval (at 18.796 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(ARD1-PadSCL)"))
    (pad SDA thru_hole oval (at 21.336 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(ARD1-PadSDA)"))
    (pad AREF thru_hole oval (at 23.876 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(ARD1-PadAREF)"))
    (pad D13 thru_hole oval (at 28.956 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(ARD1-PadD13)"))
    (pad D12 thru_hole oval (at 31.496 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(ARD1-PadD12)"))
    (pad D11 thru_hole oval (at 34.036 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(ARD1-PadD11)"))
    (pad "" thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A1 thru_hole oval (at 53.34 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(ARD1-PadA1)"))
    (pad A2 thru_hole oval (at 55.88 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(ARD1-PadA2)"))
    (pad A3 thru_hole oval (at 58.42 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(ARD1-PadA3)"))
    (pad A4 thru_hole oval (at 60.96 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(ARD1-PadA4)"))
    (pad A5 thru_hole oval (at 63.5 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "Net-(ARD1-PadA5)"))
    (pad MISO thru_hole oval (at 63.627 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "Net-(ARD1-PadMISO)"))
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E97A)
    (at 172.72 73.66)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7DB28)
    (attr smd)
    (fp_text reference D1 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E980)
    (at 172.72 81.28)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7DB63)
    (attr smd)
    (fp_text reference D2 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E986)
    (at 180.34 58.42)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7DA50)
    (attr smd)
    (fp_text reference D3 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E98C)
    (at 180.34 66.04)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7DA83)
    (attr smd)
    (fp_text reference D4 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E992)
    (at 180.34 73.66)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7DAB8)
    (attr smd)
    (fp_text reference D5 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E998)
    (at 180.34 81.28)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7DAEF)
    (attr smd)
    (fp_text reference D6 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E99E)
    (at 187.96 81.28)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D836)
    (attr smd)
    (fp_text reference D7 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9A4)
    (at 187.96 73.66)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D8AF)
    (attr smd)
    (fp_text reference D8 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9AA)
    (at 187.96 66.04)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D8EA)
    (attr smd)
    (fp_text reference D9 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9B0)
    (at 195.58 81.28)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D65C)
    (attr smd)
    (fp_text reference D10 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9B6)
    (at 195.58 73.66)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D6EF)
    (attr smd)
    (fp_text reference D11 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9BC)
    (at 195.58 66.04)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D750)
    (attr smd)
    (fp_text reference D12 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9C2)
    (at 195.58 58.42)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D7BB)
    (attr smd)
    (fp_text reference D13 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D13-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9C8)
    (at 203.2 81.28)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D90D)
    (attr smd)
    (fp_text reference D14 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D14-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9CE)
    (at 203.2 73.66)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D932)
    (attr smd)
    (fp_text reference D15 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D15-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9D4)
    (at 203.2 66.04)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D959)
    (attr smd)
    (fp_text reference D16 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D16-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9DA)
    (at 210.82 81.28)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D982)
    (attr smd)
    (fp_text reference D17 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D17-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9E0)
    (at 210.82 73.66)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D9C3)
    (attr smd)
    (fp_text reference D18 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D18-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9E6)
    (at 210.82 66.04)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7D9F0)
    (attr smd)
    (fp_text reference D19 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D19-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_PLCC-2 (layer F.Cu) (tedit 59959404) (tstamp 59B7E9EC)
    (at 210.82 58.42)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (path /59B7DA1F)
    (attr smd)
    (fp_text reference D20 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.6) (end -0.8 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.85) (end 2.5 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 -1.85) (end 2.5 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 1.85) (end -2.65 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.85) (end -2.65 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.6) (end -2.4 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.25 -1.6) (end -2.4 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.4 -1.6) (end -2.4 -0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D20-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7E9F2)
    (at 172.72 85.09 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85655)
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7E9F8)
    (at 172.72 77.47 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B856A6)
    (attr smd)
    (fp_text reference R2 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7E9FE)
    (at 180.34 85.09 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B856F3)
    (attr smd)
    (fp_text reference R3 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA04)
    (at 180.34 77.47 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85742)
    (attr smd)
    (fp_text reference R4 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA0A)
    (at 180.34 69.85 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85793)
    (attr smd)
    (fp_text reference R5 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA10)
    (at 180.34 62.23 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B857E8)
    (attr smd)
    (fp_text reference R6 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA16)
    (at 187.96 69.85 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B8583D)
    (attr smd)
    (fp_text reference R7 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA1C)
    (at 187.96 77.47 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B8589C)
    (attr smd)
    (fp_text reference R8 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D8-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA22)
    (at 187.96 85.09 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B858F5)
    (attr smd)
    (fp_text reference R9 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA28)
    (at 195.58 62.23 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85952)
    (attr smd)
    (fp_text reference R10 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D13-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA2E)
    (at 195.58 69.85 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B859B3)
    (attr smd)
    (fp_text reference R11 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D12-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA34)
    (at 195.58 77.47 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85A12)
    (attr smd)
    (fp_text reference R12 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA3A)
    (at 195.58 85.09 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85A73)
    (attr smd)
    (fp_text reference R13 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA40)
    (at 203.2 69.85 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85AD6)
    (attr smd)
    (fp_text reference R14 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D16-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R14-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA46)
    (at 203.2 77.47 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85B3D)
    (attr smd)
    (fp_text reference R15 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D15-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA4C)
    (at 203.2 85.09 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85BA6)
    (attr smd)
    (fp_text reference R16 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D14-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA52)
    (at 210.82 62.23 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85C0F)
    (attr smd)
    (fp_text reference R17 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D20-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA58)
    (at 210.82 69.85 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85C7C)
    (attr smd)
    (fp_text reference R18 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D19-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R18-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA5E)
    (at 210.82 77.47 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85CEB)
    (attr smd)
    (fp_text reference R19 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D18-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804) (tstamp 59B7EA64)
    (at 210.82 85.09 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /59B85D5C)
    (attr smd)
    (fp_text reference R20 (at 0 -1.7 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D17-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(R20-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5923F252) (tstamp 59B7EA6C)
    (at 137.16 80.01)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (path /59B845C9)
    (fp_text reference SW1 (at 3.25 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.25 2.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.25 -0.75) (end 6.25 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6.25 -0.75) (end 6.25 5.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.25 5.25) (end 0.25 5.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 5.25) (end 0.25 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.75) (end 3.25 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start 7.75 6) (end 8 6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 6) (end 8 5.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.75 -1.5) (end 8 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -1.5) (end 8 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -1.25) (end -1.5 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 5.75) (end -1.5 6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 6) (end -1.25 6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -1.5) (end 7.75 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 5.75) (end -1.5 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.75 6) (end -1.25 6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -1.25) (end 8 5.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 5.5) (end 5.5 5.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.25 1.5) (end -0.25 3) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.5 -1) (end 1 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3) (end 6.75 1.5) (layer F.SilkS) (width 0.12))
    (fp_circle (center 3.25 2.25) (end 1.25 2.5) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(ARD1-PadD8)"))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(ARD1-PadD8)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5923F252) (tstamp 59B7EA74)
    (at 153.67 81.28)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (path /59B84556)
    (fp_text reference SW2 (at 3.25 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.25 2.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.25 -0.75) (end 6.25 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6.25 -0.75) (end 6.25 5.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.25 5.25) (end 0.25 5.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 5.25) (end 0.25 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.75) (end 3.25 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start 7.75 6) (end 8 6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 6) (end 8 5.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.75 -1.5) (end 8 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -1.5) (end 8 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -1.25) (end -1.5 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 -1.5) (end -1.25 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 5.75) (end -1.5 6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 6) (end -1.25 6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -1.5) (end 7.75 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.5 5.75) (end -1.5 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.75 6) (end -1.25 6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8 -1.25) (end 8 5.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 5.5) (end 5.5 5.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.25 1.5) (end -0.25 3) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.5 -1) (end 1 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.75 3) (end 6.75 1.5) (layer F.SilkS) (width 0.12))
    (fp_circle (center 3.25 2.25) (end 1.25 2.5) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(ARD1-PadD9)"))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(ARD1-PadD9)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )

  (module SMD_Packages:SO-16-L (layer F.Cu) (tedit 0) (tstamp 59B7EA88)
    (at 176.53 92.202 90)
    (path /59B7FC4D)
    (attr smd)
    (fp_text reference U1 (at 0 1.524 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 74HC595 (at 0.381 -1.905 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.08 4.191) (end -5.08 4.191) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 4.191) (end -5.08 -4.191) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -4.191) (end 5.08 -4.191) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -4.191) (end 5.08 4.191) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -0.635) (end -4.318 -0.635) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.318 -0.635) (end -4.318 0.635) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.318 0.635) (end -5.08 0.635) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.445 5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -3.175 5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -1.905 5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R4-Pad2)"))
    (pad 4 smd rect (at -0.635 5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R5-Pad2)"))
    (pad 5 smd rect (at 0.635 5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R6-Pad2)"))
    (pad 6 smd rect (at 1.905 5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at 3.175 5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 4.445 5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at 4.445 -5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 3.175 -5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 11 smd rect (at 1.905 -5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(ARD1-PadD3)"))
    (pad 12 smd rect (at 0.635 -5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(ARD1-PadD4)"))
    (pad 13 smd rect (at -0.635 -5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 14 smd rect (at -1.905 -5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(ARD1-PadD2)"))
    (pad 15 smd rect (at -3.175 -5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R1-Pad2)"))
    (pad 16 smd rect (at -4.445 -5.08 90) (size 0.635 1.905) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model SMD_Packages.3dshapes/SO-16-L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.6 0.5))
      (rotate (xyz 0 0 0))
    )
  )

  (module SMD_Packages:SO-16-L (layer B.Cu) (tedit 0) (tstamp 59B7EA9C)
    (at 191.77 97.79 180)
    (path /59B7FAFF)
    (attr smd)
    (fp_text reference U2 (at 0 -1.524 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 74HC595 (at 0.381 1.905 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 5.08 -4.191) (end -5.08 -4.191) (layer B.SilkS) (width 0.15))
    (fp_line (start -5.08 -4.191) (end -5.08 4.191) (layer B.SilkS) (width 0.15))
    (fp_line (start -5.08 4.191) (end 5.08 4.191) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.08 4.191) (end 5.08 -4.191) (layer B.SilkS) (width 0.15))
    (fp_line (start -5.08 0.635) (end -4.318 0.635) (layer B.SilkS) (width 0.15))
    (fp_line (start -4.318 0.635) (end -4.318 -0.635) (layer B.SilkS) (width 0.15))
    (fp_line (start -4.318 -0.635) (end -5.08 -0.635) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.445 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(R8-Pad2)"))
    (pad 2 smd rect (at -3.175 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(R9-Pad2)"))
    (pad 3 smd rect (at -1.905 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(R10-Pad2)"))
    (pad 4 smd rect (at -0.635 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(R11-Pad2)"))
    (pad 5 smd rect (at 0.635 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(R12-Pad2)"))
    (pad 6 smd rect (at 1.905 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(R13-Pad2)"))
    (pad 7 smd rect (at 3.175 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at 4.445 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 9 smd rect (at 4.445 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 3.175 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 9 VCC))
    (pad 11 smd rect (at 1.905 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(ARD1-PadD6)"))
    (pad 12 smd rect (at 0.635 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(ARD1-PadD7)"))
    (pad 13 smd rect (at -0.635 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 14 smd rect (at -1.905 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(ARD1-PadD5)"))
    (pad 15 smd rect (at -3.175 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(R7-Pad2)"))
    (pad 16 smd rect (at -4.445 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 9 VCC))
    (model SMD_Packages.3dshapes/SO-16-L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.6 0.5))
      (rotate (xyz 0 0 0))
    )
  )

  (module SMD_Packages:SO-16-L (layer B.Cu) (tedit 0) (tstamp 59B7EAB0)
    (at 208.28 97.79 180)
    (path /59B7FBFE)
    (attr smd)
    (fp_text reference U3 (at 0 -1.524 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 74HC595 (at 0.381 1.905 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 5.08 -4.191) (end -5.08 -4.191) (layer B.SilkS) (width 0.15))
    (fp_line (start -5.08 -4.191) (end -5.08 4.191) (layer B.SilkS) (width 0.15))
    (fp_line (start -5.08 4.191) (end 5.08 4.191) (layer B.SilkS) (width 0.15))
    (fp_line (start 5.08 4.191) (end 5.08 -4.191) (layer B.SilkS) (width 0.15))
    (fp_line (start -5.08 0.635) (end -4.318 0.635) (layer B.SilkS) (width 0.15))
    (fp_line (start -4.318 0.635) (end -4.318 -0.635) (layer B.SilkS) (width 0.15))
    (fp_line (start -4.318 -0.635) (end -5.08 -0.635) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.445 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(R15-Pad2)"))
    (pad 2 smd rect (at -3.175 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(R16-Pad2)"))
    (pad 3 smd rect (at -1.905 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(R17-Pad2)"))
    (pad 4 smd rect (at -0.635 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(R18-Pad2)"))
    (pad 5 smd rect (at 0.635 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(R19-Pad2)"))
    (pad 6 smd rect (at 1.905 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(R20-Pad2)"))
    (pad 7 smd rect (at 3.175 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at 4.445 -5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 9 smd rect (at 4.445 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(U3-Pad9)"))
    (pad 10 smd rect (at 3.175 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 9 VCC))
    (pad 11 smd rect (at 1.905 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(ARD1-PadD11)"))
    (pad 12 smd rect (at 0.635 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(ARD1-PadD12)"))
    (pad 13 smd rect (at -0.635 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 14 smd rect (at -1.905 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(ARD1-PadD10)"))
    (pad 15 smd rect (at -3.175 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(R14-Pad2)"))
    (pad 16 smd rect (at -4.445 5.08 180) (size 0.635 1.905) (layers B.Cu B.Paste B.Mask)
      (net 9 VCC))
    (model SMD_Packages.3dshapes/SO-16-L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.6 0.5))
      (rotate (xyz 0 0 0))
    )
  )

  (segment (start 174.22 73.66) (end 174.22 77.32) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 174.22 77.32) (end 174.07 77.47) (width 0.25) (layer F.Cu) (net 36) (tstamp 59B7EFE8))
  (segment (start 174.22 81.28) (end 174.22 84.94) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 174.22 84.94) (end 174.07 85.09) (width 0.25) (layer F.Cu) (net 37) (tstamp 59B7EFEB))
  (segment (start 181.84 58.42) (end 181.84 62.08) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 181.84 62.08) (end 181.69 62.23) (width 0.25) (layer F.Cu) (net 38) (tstamp 59B7F031))
  (segment (start 181.84 66.04) (end 181.84 69.7) (width 0.25) (layer F.Cu) (net 39))
  (segment (start 181.84 69.7) (end 181.69 69.85) (width 0.25) (layer F.Cu) (net 39) (tstamp 59B7EFFD))
  (segment (start 181.84 73.66) (end 181.84 77.32) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 181.84 77.32) (end 181.69 77.47) (width 0.25) (layer F.Cu) (net 40) (tstamp 59B7EFF1))
  (segment (start 181.84 81.28) (end 181.84 84.94) (width 0.25) (layer F.Cu) (net 41))
  (segment (start 181.84 84.94) (end 181.69 85.09) (width 0.25) (layer F.Cu) (net 41) (tstamp 59B7EFEE))
  (segment (start 189.46 81.28) (end 189.46 84.94) (width 0.25) (layer F.Cu) (net 42))
  (segment (start 189.46 84.94) (end 189.31 85.09) (width 0.25) (layer F.Cu) (net 42) (tstamp 59B7F018))
  (segment (start 189.46 73.66) (end 189.46 77.32) (width 0.25) (layer F.Cu) (net 43))
  (segment (start 189.46 77.32) (end 189.31 77.47) (width 0.25) (layer F.Cu) (net 43) (tstamp 59B7EFF4))
  (segment (start 189.46 66.04) (end 189.46 69.7) (width 0.25) (layer F.Cu) (net 44))
  (segment (start 189.46 69.7) (end 189.31 69.85) (width 0.25) (layer F.Cu) (net 44) (tstamp 59B7EFFA))
  (segment (start 197.08 81.28) (end 197.08 84.94) (width 0.25) (layer F.Cu) (net 45))
  (segment (start 197.08 84.94) (end 196.93 85.09) (width 0.25) (layer F.Cu) (net 45) (tstamp 59B7F00F))
  (segment (start 197.08 73.66) (end 197.08 77.32) (width 0.25) (layer F.Cu) (net 46))
  (segment (start 197.08 77.32) (end 196.93 77.47) (width 0.25) (layer F.Cu) (net 46) (tstamp 59B7EFF7))
  (segment (start 197.08 66.04) (end 197.08 69.7) (width 0.25) (layer F.Cu) (net 47))
  (segment (start 197.08 69.7) (end 196.93 69.85) (width 0.25) (layer F.Cu) (net 47) (tstamp 59B7F000))
  (segment (start 197.08 58.42) (end 197.08 62.08) (width 0.25) (layer F.Cu) (net 48))
  (segment (start 197.08 62.08) (end 196.93 62.23) (width 0.25) (layer F.Cu) (net 48) (tstamp 59B7F01E))
  (segment (start 204.7 81.28) (end 204.7 84.94) (width 0.25) (layer F.Cu) (net 49))
  (segment (start 204.7 84.94) (end 204.55 85.09) (width 0.25) (layer F.Cu) (net 49) (tstamp 59B7F012))
  (segment (start 204.7 73.66) (end 204.7 77.32) (width 0.25) (layer F.Cu) (net 50))
  (segment (start 204.7 77.32) (end 204.55 77.47) (width 0.25) (layer F.Cu) (net 50) (tstamp 59B7F00C))
  (segment (start 204.7 66.04) (end 204.7 69.7) (width 0.25) (layer F.Cu) (net 51))
  (segment (start 204.7 69.7) (end 204.55 69.85) (width 0.25) (layer F.Cu) (net 51) (tstamp 59B7F003))
  (segment (start 212.32 81.28) (end 212.32 84.94) (width 0.25) (layer F.Cu) (net 52))
  (segment (start 212.32 84.94) (end 212.17 85.09) (width 0.25) (layer F.Cu) (net 52) (tstamp 59B7F015))
  (segment (start 212.32 73.66) (end 212.32 77.32) (width 0.25) (layer F.Cu) (net 53))
  (segment (start 212.32 77.32) (end 212.17 77.47) (width 0.25) (layer F.Cu) (net 53) (tstamp 59B7F009))
  (segment (start 212.32 66.04) (end 212.32 69.7) (width 0.25) (layer F.Cu) (net 54))
  (segment (start 212.32 69.7) (end 212.17 69.85) (width 0.25) (layer F.Cu) (net 54) (tstamp 59B7F006))
  (segment (start 212.32 58.42) (end 212.32 62.08) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 212.32 62.08) (end 212.17 62.23) (width 0.25) (layer F.Cu) (net 55) (tstamp 59B7F01B))
  (segment (start 171.37 85.09) (end 170.053 85.09) (width 0.25) (layer F.Cu) (net 56) (status 400000))
  (segment (start 169.926 95.377) (end 171.45 95.377) (width 0.25) (layer F.Cu) (net 56) (tstamp 59B7F219) (status 800000))
  (segment (start 169.545 94.996) (end 169.926 95.377) (width 0.25) (layer F.Cu) (net 56) (tstamp 59B7F218))
  (via (at 169.545 94.996) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 56))
  (segment (start 169.545 85.598) (end 169.545 94.996) (width 0.25) (layer B.Cu) (net 56) (tstamp 59B7F215))
  (via (at 169.545 85.598) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 56))
  (segment (start 170.053 85.09) (end 169.545 85.598) (width 0.25) (layer F.Cu) (net 56) (tstamp 59B7F212))
  (segment (start 181.61 96.647) (end 173.355 96.647) (width 0.25) (layer F.Cu) (net 57) (status 400000))
  (segment (start 173.355 78.867) (end 171.958 77.47) (width 0.25) (layer F.Cu) (net 57) (tstamp 59B7F20E) (status 800000))
  (via (at 173.355 78.867) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 57))
  (segment (start 173.355 96.647) (end 173.355 78.867) (width 0.25) (layer B.Cu) (net 57) (tstamp 59B7F20B))
  (via (at 173.355 96.647) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 57))
  (segment (start 171.958 77.47) (end 171.37 77.47) (width 0.25) (layer F.Cu) (net 57) (tstamp 59B7F20F) (status C00000))
  (segment (start 181.61 95.377) (end 177.673 95.377) (width 0.25) (layer F.Cu) (net 58))
  (segment (start 177.8 85.09) (end 178.99 85.09) (width 0.25) (layer F.Cu) (net 58) (tstamp 59B7F1DC))
  (segment (start 177.673 85.217) (end 177.8 85.09) (width 0.25) (layer F.Cu) (net 58) (tstamp 59B7F1DB))
  (via (at 177.673 85.217) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 58))
  (segment (start 177.673 95.377) (end 177.673 85.217) (width 0.25) (layer B.Cu) (net 58) (tstamp 59B7F1D8))
  (via (at 177.673 95.377) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 58))
  (segment (start 181.61 94.107) (end 177.038 94.107) (width 0.25) (layer F.Cu) (net 59))
  (segment (start 177.292 77.47) (end 178.99 77.47) (width 0.25) (layer F.Cu) (net 59) (tstamp 59B7F1F3))
  (segment (start 177.038 77.724) (end 177.292 77.47) (width 0.25) (layer F.Cu) (net 59) (tstamp 59B7F1F2))
  (via (at 177.038 77.724) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 59))
  (segment (start 177.038 94.107) (end 177.038 77.724) (width 0.25) (layer B.Cu) (net 59) (tstamp 59B7F1EF))
  (via (at 177.038 94.107) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 59))
  (segment (start 178.562 77.47) (end 178.99 77.47) (width 0.25) (layer F.Cu) (net 59) (tstamp 59B7F116))
  (segment (start 181.61 92.837) (end 176.403 92.837) (width 0.25) (layer F.Cu) (net 60))
  (segment (start 176.657 69.85) (end 178.99 69.85) (width 0.25) (layer F.Cu) (net 60) (tstamp 59B7F1FC))
  (segment (start 176.403 70.104) (end 176.657 69.85) (width 0.25) (layer F.Cu) (net 60) (tstamp 59B7F1FB))
  (via (at 176.403 70.104) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 60))
  (segment (start 176.403 92.837) (end 176.403 70.104) (width 0.25) (layer B.Cu) (net 60) (tstamp 59B7F1F8))
  (via (at 176.403 92.837) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 60))
  (segment (start 181.61 91.567) (end 175.768 91.567) (width 0.25) (layer F.Cu) (net 61))
  (segment (start 176.022 62.23) (end 178.99 62.23) (width 0.25) (layer F.Cu) (net 61) (tstamp 59B7F205))
  (segment (start 175.768 62.484) (end 176.022 62.23) (width 0.25) (layer F.Cu) (net 61) (tstamp 59B7F204))
  (via (at 175.768 62.484) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 61))
  (segment (start 175.768 91.567) (end 175.768 62.484) (width 0.25) (layer B.Cu) (net 61) (tstamp 59B7F201))
  (via (at 175.768 91.567) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 61))

)
