# /home/enbewe/Coding/KiCad/ESP8266-WS2812-Puck/ESP8266-WS2812-Puck.sch

Do 14 Okt 2021 14:01:31 CEST

Eeschema 5.1.10-88a1d61d58~90~ubuntu20.04.1

Component Count:28

Ref | Qnty | Value | Part | Datasheet | Description | Vendor
--- | --- | --- | --- | --- | --- | ---
C1, C2, C5 | 3 | 10uF | Device:C | ~ | Unpolarized capacitor |
C3, C6 | 2 | 100nF | Device:C | ~ | Unpolarized capacitor |
C4 | 1 | 100uF | Device:CP1 | ~ | Polarized capacitor, US symbol |
D1 | 1 | SS14 | Diode:1N5819 | http://www.vishay.com/docs/88525/1n5817.pdf | 40V 1A Schottky Barrier Rectifier Diode, DO-41 |
J1 | 1 | WS2812-Strip | Connector:Conn_01x04_Female | ~ | Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/) |
J2 | 1 | OLED | Connector:Conn_01x04_Female | ~ | Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/) |
P1 | 1 | USB_C_Plug_USB2.0 | Connector:USB_C_Plug_USB2.0 | https://www.usb.org/sites/default/files/documents/usb_type-c.zip | USB 2.0-only Type-C Plug connector |
Q1, Q2 | 2 | S8050 | s8050_Mod:S8050 | http://www.unisonic.com.tw/datasheet/S8050.pdf | 0.7A Ic, 20V Vce, Low Voltage High Current NPN Transistor, TO-92 |
R1, R5, R6, R7, R8, R9, R12, R13 | 8 | 12k | Device:R | ~ | Resistor |
R2, R3 | 2 | 5k1 | Device:R | ~ | Resistor |
R10, R11 | 2 | 470 | Device:R | ~ | Resistor |
SW1 | 1 | SW_SPST | Switch:SW_SPST | ~ | Single Pole Single Throw (SPST) switch |
U1 | 1 | ESP-12E | RF_Module:ESP-12E | http://wiki.ai-thinker.com/_media/esp8266/esp8266_series_modules_user_manual_v1.1.pdf | 802.11 b/g/n Wi-Fi Module |
U2 | 1 | LM1117-3.3 | Regulator_Linear:LM1117-3.3 | http://www.ti.com/lit/ds/symlink/lm1117.pdf | 800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223 |
U3 | 1 | CH340C | Interface_USB:CH340C | https://datasheet.lcsc.com/szlcsc/Jiangsu-Qin-Heng-CH340C_C84681.pdf | USB serial converter, UART, SOIC-16 |