(module Resonator_SMD_muRata_CSTCC-3pin_3.2x1.3mm_HandSoldering (layer F.Cu) (tedit 5AFDA5F1)
  (descr "SMD Resomator/Filter Murata SFECV, http://cdn-reichelt.de/documents/datenblatt/B400/SFECV-107.pdf, hand-soldering, 6.9x2.9mm^2 package")
  (tags "SMD SMT ceramic resonator filter filter hand-soldering")
  (attr smd)
  (fp_text reference REF** (at 0 0) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_text value Resonator_SMD_muRata_CSTCC-3pin_3.2x1.3mm_HandSoldering (at 0 2.4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 -2.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
  (fp_line (start -1.6 0.65) (end 1.6 0.65) (layer F.Fab) (width 0.1))
  (fp_line (start 1.6 0.65) (end 1.6 -0.65) (layer F.Fab) (width 0.1))
  (fp_line (start 1.6 -0.65) (end -1.6 -0.65) (layer F.Fab) (width 0.1))
  (fp_line (start -1.6 0) (end -0.95 0.65) (layer F.Fab) (width 0.1))
  (fp_line (start -2.2 -1.5) (end -2.2 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.2 1.5) (end 2.2 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.3 -1.6) (end -2.3 1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.3 1.6) (end 2.3 1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.3 1.6) (end 2.3 -1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.3 -1.6) (end -2.3 -1.6) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -1.2 0) (size 0.4 2.1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 0) (size 0.4 2.1) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 1.2 0) (size 0.4 2.1) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Crystals.3dshapes/Resonator_SMD_muRata_SFECV-3pin_6.9x2.9mm_HandSoldering.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
